1.5       first slit opening (mm)
0.6       second slit opening
15.0      sample length
1500.0    distance from first slit to sample
500.0     distance from second slit to sample

16x10b_7.uu.ref
69	ndata_pp
16x10b_7.dd.ref
69	ndata_mm
16x10b_7.ud.ref
69	ndata_pm
16x10b_7.du.ref
69	ndata_mp

4.52       wavelength (in Angstroem)
0.021      rms (in A)  0.021

1         number of layers on top of the multilayer

35.0     thickness in (A)                         | Al203	 150                    	1
5.7      real part of nuclear scattering length density Nb'  (in A**-2) *1e6            2
2.3d-4  imaginary part of nuclear scattering length density Nb'' (in A**-2) *1e6        3
0.0      magnetic scattering length density Np (in A**-2) *1e6                          4
90.0     theta [deg.] (0 on z, 90 on x-y plane)					        5
90.0     phi [deg.]  (0 on x, 90 on y)						        6
3.0      sigma (in A)								        7

2        number of layers in the (magnetic) unit cell

18.8     thickness in (A)                         | CoFe                                 8
1.3      real part of nuclear scattering length density Nb'  (in A**-2) *1e6             9
3.3d-4  imaginary part of nuclear scattering length density Nb'' (in A**-2) *1e6        10
2.0     magnetic scattering length density Np (in A**-2) *1e6                           11
90.0     theta [deg.] (0 on z, 90 on x-y plane)					        12
90.0     phi [deg.]  (0 on x, 90 on y)						        13
3.0      sigma (in A)								        14

35.0     thickness in (A)                         | Al203	 150                            15
5.7      real part of nuclear scattering length density Nb'  (in A**-2) *1e6            16
2.3d-4  imaginary part of nuclear scattering length density Nb'' (in A**-2) *1e6        17
0.0      magnetic scattering length density Np (in A**-2) *1e6                          18
90.0     theta [deg.] (0 on z, 90 on x-y plane)					        19
90.0     phi [deg.]  (0 on x, 90 on y)						        20
3.0      sigma (in A)								        21

10      number of such cell in the multilayer stack

0       number of layers below the multilayer stack

5.7      substrate's real part of nuclear scattering length density Nb'  (in A**-2) *1e6  | Glass   22
9.77d-3  substrate's Nb'' imaginary part of nuclear scattering length density Nb'' (in A**-2) *1e6  23
0.0      magnetic scattering length density Np (in A**-2) *1e6                                      24
90.0     theta [deg.] (0 on z, 90 on x-y plane)					                    25
90.0     phi [deg.]  (0 on x, 90 on y)						                    26
4.0      sigma (in A)								                    27

15.0     scaling factor	28
10.0      background		29

0.94	   polarizer efficiency			30
0.94      analyzer efficiency (makes +)		32
1.00       first flipper efficiency		33
1.00      second flipper efficiency		34

0          1/0 for fit or simulation

4          number of fitted parameters
2  9 11  16
     
1       	number of constraint equalities
2 	         number of parameters to be kept equal     
2 16           	list of those parameters

0.001      alamda_first
1          ntest



2          number of parameters to be kept equal     
1 15           list of those parameters




